  NEMESIS.CPX by JAY Software (18.12.1998)
陳様様様様様様様様様様様様様様様様様様様様陳

When I have installed the Nemesis accelerator from the Black Scorpion 
Software to my Falcon030, I found, that in pack weren't CPX or accessory
for controling this powerfull board. There were only TTP programs. So 
I have written this CPX.

You can switch either the NEMESIS frequences (buttons Nemesis Hi and
Nemesis Lo) or standard frequences (16 MHz or 8 MHz). In case the Nemesis
is not installed you can use only these 'low' options.

The next function of this CPX is controling the processor caches. You
can switch both data and instruction cache independently.

In Info section you can find curently running resolution, and versions
of system components.

This CPX module is FREEWARE, that mean you could freely copy it, until
they are all original files in a pack.


Authors don't take responsibility to damages caused by this program !!!


  All comments, suggestions, donations, additional information, etc. 
                 are welcome at any of our addresses:


               JAY Software

               Jan Krupka      or       Stanislav Opichal
               Trnkova 26               Za Vodojemem 8
               Olomouc                  Olomouc
               779 00                   779 00
               Czech Republic           Czech Republic

         tel.: +420 068 5419108
       e-mail: krupkaj@risc.upol.cz     opichals@risc.upol.cz
      fidonet: 2:421/70.15

          www: html://www.inf.upol.cz/~opichals/jay
